New environment settings

Regarding the new boards MT7620-2077 I found that they lack basic support for wifi operation in the WDS mode, that is because it didn’t have neither the ‘iw’ nor the ‘hostapd’ package. Here’s the procedure:

1. Flash the image with the packages
2. Configure the image following the instructions file
3. Prepare a check/control script

The package iw was needed to have the scan feature so that with luci we can see the wifi usage and we can see other wifi networks and connect to them easily. If you install more than one wifi handler you’ll get messy!! Most importantly don’t install too many libraries all at once, I needed the symbolic but got me 2 more wifi interfaces.